**2.3.2 Gutter Dam**

**Operation and Site Condition:** An inlet is located at the bottom of the cul-de-sac which is at a roadway sag. Inlet protection can cause flooding and will likely damaged adjacent residential property. Therefore a gutter dam has been selected to be a redundant BMP to the other sediment control BMPs. This BMP is designed with dual catchments so performance can be measured. A property maintained gutter dam and the other erosion boundary control BMPs should be sufficient for this size of project.

**Instruction:** Install 6” dia ¾” gravel filled bag filters installed per detail and site plan. Do drive on or park over this BMP.

**Installation Schedule:** Prior to any land disturbance

**Maintenance Requirements:** Maintain per the minimum.

**Applicable Trades:** NA

**Maintenance Personnel:** Project Manager. Any trade damaging this BMP is expected to prepare or replace it

**Detail:**

