**2.3.4 Manual Sweeping**

**Operation and Site Conditions:** Some operations require driving off durable surfaces and the track out or boundary controls can fail which will necessitate cleaning of the streets and gutters.

**Instruction:** Square nose shovel and broom. All trades are expected to remove tracked out or mud and dirt that end up on street from regular operations. Repeat removal until no more mud can be picked up. Do not worry about the dirt stain and do not wash with water. The small amounts of mud trapped in the tread will also spread dirt on the streets overtime. In this case the mud will be removed by BMP 2.3.3.

**Schedule:** NA.

**Maintenance:** Immediately following the incident. Minor track out not causing a public nuisance and no risk of being washed to stormwater systems may be removed at end of day or before forecast storm event whichever comes first.

**Maintenance Personnel:** Any trade tracking the mud

**Applicable Trades:** All

**Detail:** NA