**2.4.1 Hose**

**Operation or Site Condition:** Excavation, grading and even other normal construction activity will kick up dust on hot windy days.

**Instruction:** Garden hose provided for construction operations kicking up dust or other activities involving light weight powdery materials.

**Installation Schedule:** Provide hose connected to a culinary water jumper from City Water Department prior to land disturbance.

**Maintenance:** Generally, apply during excavation, grading and mortar mixing operations. Also prior to end of work day ground is powdery.

**Maintenance Personnel:** Project Manager will watch for general dry dusty conditions. However, each trade will be expected to use this BMP for operations they are responsible for. Primarily for excavation, grading and Brick Mason operations however any trade kicking up dust is expected to implement this BMP.

**Applicable Trades:** Primarily Excavator, Grader and Brick Masons but also any trade whose operation is kicking up dust.

**Detail:** NA