**2.7.2 Utility Backfill Staging Zone**

**Operation or Site Conditions:** Sewer pipe installation, Power connection, Phone connection, and Gas connection.

**Instruction:** Utility Companies and Plumbers stage your backfill next to each other as shown on the site Plan. A location just off the parking pad is provided where you will be able to access your backfill without tracking mud onto the street. See location and staging envelope on Site Plans in Appendix B

**Schedule:** NA

**Maintenance:** NA

**Maintenance Personnel:** NA

**Applicable Trades:** Primarily Plumber X, Rocky Mountain Power, Centurylink, Comcast and Questar

**Detail:** NA