**2.5.2 Parking Pad**

**Operation or Site Condition:** Most tradesmen will need to enter and exit the site either to transport tools or supplies. The parking pad system intended to prevent mud from sticking to tires or tracks.

**Instruction:** All tradesmen are required to park on the parking pad or the street except for the tradesmen authorized by me to drive off the pad. Any trades with mud on tires must apply BMP 2.5.1. The forklift, excavator, skid-steer operators are the only persons allowed off the pad, however, they are required to apply BMP 2.5.1 and 2.3.4 as part of their normal operation. Do not allow mud to remain on the road as you will be required to scrape and broom it manually.

**Installation Schedule:** Following backfill of foundation

**Maintenance Requirements:** Replace gravel or rake when mud or dirt is sticking to tires

**Applicable Trades:** All trades driving onto the site

**Maintenance Personnel:** Project Manager. Inform me if you notice any problems.

**Detail:**

