**2.6.6 Dirt Gutter Dams**

**Operation or Site Condition:** Concrete cutting is necessary for the 20’ wide drive approach. The cutter will be using coolant necessitating containment.

**Instruction:** Concrete Cutting Company X, build a 18”wide 24” long dirt gutter dam enough to contain coolant and cutting slurry. Remove dirt and cutting slurry immediately following the cut. Broom until no more material can be picked up with a square nose shovel. Dispose of waste in BMP 2.6.5.

**Schedule:** Prior to concrete cutting operation

**Maintenance:** NA

**Maintenance Personnel:** NA

**Applicable Trades:** Concrete Cutting Company X

**Detail:** NA