**City Site Conditions and Maintenance Minimums**

**General**

***Minimum:***Repair damaged BMPs with-in 7 days and prior to forecast precipitation and non-stormwater runoff and whichever comes first.

**Track Out**

***Minimum:*** *Remove all mud or dirt by the end of each work day, and when track out amounts become a hazard, unacceptable public nuisances or before wet conditions whichever, comes first. Performance: No more material can be removed with square nose shove and broom.*

**Inlet Control**

***Minimum:***Remove sediment at the end of each workday, or before a forecast storm event which comes first.

**Clean up**

***Minimum:***Removal of mud, dirt, trash and other debris is necessary but cannot be accepted to replace the prevention BMPs.