Approved Standard Installation Drawings & Specifications (New) versus Plan Submittal Waiver (Old)

|  |  |  |
| --- | --- | --- |
|  | **Approved Standard Installation Drawings and Specifications for Water Lines**  [Rule R309-500-7, Effective 11/7/2017] | **Plan Submittal Waiver**  [Expired on 11/7/2017] |
| 1 | A **single** approval | Two waiver types (3)(a) & (3)(b) |
| 2 | Master Plan-based approval **unavailable** | (3)(a) Master Plan-based waiver available |
| 3 | Diameter of water lines eligible(≤16”) **regardless population served** | (3)(b) Diameter of water lines eligible for waivers based on population served |
| 4 | PWS must submit application for approved Standard Installation Drawings and Specs | PWS must obtain waiver eligibility |
| 5 | **Approval must be renewed every 5 years** (or whenever standard drawings and specs change) | Waiver eligibility does not expire |
| 6 | **Required for approval:**   1. **Application form** (available from DDW) 2. Standard installation drawings and specs **(with effective date)** meeting R309-550 requirements 3. PE designation for system design by PWS (notify DDW of change) 4. PE designation for hydraulic analysis by PWS (notify DDW of change)   Statement acknowledging: (1) hydraulic analysis and (2) flushing, disinfection, coliform sampling, as-built drawings **with application only** | Required for waiver eligibility:   1. Letter requesting eligibility 2. Standard installation drawings and specs meeting R309-550 3. PE designation for system design by PWS [(3)(b)] 4. PE designation for hydraulic analysis by PWS [(3)(b)]   Certification by designated PEs for (1) hydraulic analysis and (2) flushing, disinfection, coliform sampling, as-built drawings for each waiver request |
| 7 | Project Notification Form (PNF) and waiver request **not required** | Submit PNF with each waiver request |
| 8 | **Not required** | Obtain waiver for each water line project prior to construction (3a & 3b) |
| 9 | **Not required** | May obtain year-end after-the-fact waiver for multiple water line projects (3b) |
| 10 | **Not required** | Maintain a tracking sheet for year-end, after-the-fact waivers (3)(b) |
| 11 | (Same) | **Pump stations ineligible** for waivers |
| 12 | (Same) | Water **lines >16” ineligible** for waivers |
| 13 | (Same) | Water line **projects not meeting water/sewer separation must obtain exception** to R309-550-7 |