|  |  |
| --- | --- |
| **Facility Name**  | **Facility ID**  |
| **Address**  | **Tester’s Name**  |
|  | **Test Date**  | **Phone**  |
|  |
| **Tank number** |       |       |       |       |       |       |
| **Product Stored** |       |       |       |       |       |       |
| **Capacity** |       |       |       |       |       |       |
| **Manufacturer** |       |       |       |       |       |       |
| **Construction** |  [ ]  Single walled [ ]  Double walled | [ ]  Single walled[ ]  Double walled | [ ]  Single walled[ ]  Double walled | [ ]  Single walled[ ]  Double walled | [ ]  Single walled[ ]  Double walled | [ ]  Single walled[ ]  Double walled |
| **Liquid and debris removed** |  [ ]  Yes  [ ]  No | [ ]  Yes [ ]  No | [ ]  Yes[ ]  No | [ ]  Yes [ ]  No | [ ]  Yes [ ]  No | [ ]  Yes [ ]  No |
| **Visual Inspection****No cracks, holes or separations.** |  [ ]  Pass  [ ]  Fail  | [ ]  Pass [ ]  Fail | [ ]  Pass [ ]  Fail | [ ]  Pass [ ]  Fail | [ ]  Pass [ ]  Fail | [ ]  Pass [ ]  Fail |
| **Tank riser cap included in test?** |  [ ]  Yes  [ ]  No | [ ]  Yes [ ]  No | [ ]  Yes[ ]  No | [ ]  Yes [ ]  No | [ ]  Yes [ ]  No | [ ]  Yes [ ]  No |
| **Is drain valve included in test?** |  [ ]  Yes  [ ]  No  [ ]  N/A |  [ ]  Yes  [ ]  No  [ ]  N/A |  [ ]  Yes  [ ]  No  [ ]  N/A |  [ ]  Yes  [ ]  No  [ ]  N/A |  [ ]  Yes  [ ]  No  [ ]  N/A |  [ ]  Yes  [ ]  No  [ ]  N/A |
| **Start Level** |       |       |       |       |       |       |
| **Start Time** |       |       |       |       |       |       |
| **Ending Level** |       |       |       |       |       |       |
| **End Time** |       |       |       |       |       |       |
| **Test Period(Minimum of 1 hour)**  |       |       |       |       |       |       |
| **Change in Level** |       |       |       |       |       |       |
| **Test Results** |  [ ]  Pass  [ ]  Fail  |  [ ]  Pass  [ ]  Fail |  [ ]  Pass  [ ]  Fail |  [ ]  Pass  [ ]  Fail |  [ ]  Pass  [ ]  Fail |  [ ]  Pass  [ ]  Fail |
| **Photos indicating water levels are attached?** | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  |
| **Pass/fail criteria: Must pass visual inspection, test duration at least one hour, must include photos with this form, water level drop of less than 1/8 inch. Ref: PEI/RP 1200 6.2.5 Test Procedure** |
| **How was the liquid disposed?**       |
| **Comments**      |

I certify under penalty of law that the above information is true, accurate and complete.

Aug 2016

**Tester’s Signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**