|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Facility Name** | | | | | | **Facility ID** | | |
| **Address** | | | **Tester’s Name** | | | | | |
|  | | | **Test Date** | | | **Phone** | | |
|  | | | | | | | | |
| **Tank number** |  |  | |  |  | |  |  |
| **Product Stored** |  |  | |  |  | |  |  |
| **Capacity** |  |  | |  |  | |  |  |
| **Manufacturer** |  |  | |  |  | |  |  |
| **Construction** | Single walled  Double walled | Single walled  Double walled | | Single walled  Double walled | Single walled  Double walled | | Single walled  Double walled | Single walled  Double walled |
| **Liquid and debris removed** | Yes  No | Yes  No | | Yes  No | Yes  No | | Yes  No | Yes  No |
| **Visual Inspection**  **No cracks, holes or separations.** | Pass  Fail | Pass   Fail | | Pass   Fail | Pass   Fail | | Pass   Fail | Pass   Fail |
| **Tank riser cap included in test?** | Yes  No | Yes  No | | Yes  No | Yes  No | | Yes  No | Yes  No |
| **Is drain valve included in test?** | Yes  No  N/A | Yes  No  N/A | | Yes  No  N/A | Yes  No  N/A | | Yes  No  N/A | Yes  No  N/A |
| **Start Level** |  |  | |  |  | |  |  |
| **Start Time** |  |  | |  |  | |  |  |
| **Ending Level** |  |  | |  |  | |  |  |
| **End Time** |  |  | |  |  | |  |  |
| **Test Period (Minimum of 1 hour)** |  |  | |  |  | |  |  |
| **Change in Level** |  |  | |  |  | |  |  |
| **Test Results** | Pass  Fail | Pass  Fail | | Pass  Fail | Pass  Fail | | Pass  Fail | Pass  Fail |
| **Photos indicating water levels are attached?** |  |  | |  |  | |  |  |
| **Pass/fail criteria: Must pass visual inspection, test duration at least one hour, must include photos with this form, water level drop of less than 1/8 inch. Ref: PEI/RP 1200 6.2.5 Test Procedure** | | | | | | | | |
| **How was the liquid disposed?** | | | | | | | | |
| **Comments** | | | | | | | | |

I certify under penalty of law that the above information is true, accurate and complete.

Aug 2016

**Tester’s Signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**