**2.2.1 Steel Plate and Marker**

**Operations or Site Condition:** An irrigation well exists on this property near the rear property boundary. Informing the workforce will be sufficient to protect this irrigation well from damage or contamination.

**Instruction:** Install a ¼” steel plate and marker. Do not bury.

**Installation Schedule:** Prior to any land disturbance

**Maintenance Requirements:** Repair if damaged

**Maintenance Personnel:** Project Manager

**Applicable Trades:** Excavator and grading subs

**Detail:** NA