**2.5.3 Forklift Policy**

**Operation or Site Condition:** Forklift operators will need to enter and travel on the road to reach the north, west and south sides of the home.

**Instruction:** Forklift operator must stop the vehicle immediately after crossing back over the curb and remove any mud chunks from the road. To prevent the hassle of removing mud, it will be best if you schedule your Forklift operations during dry weather. The manual sweeping will need to meet the requirements in BMP 2.3.4 Manual Sweeping.

**Installation Schedule:** NA

**Maintenance Requirements:** Upon incident

**Applicable Trades:** Framer Co. x, Drywall Co. x, Landscape Co. x

**Maintenance Personnel:** Forklift Operator

**Detail:** NA