**2.5.1 Scrape Tires**

**Operation or Site Condition:** It is not practical to provide a parking pad for the excavation, forklift and final grade operations, therefore it is necessary to scrape tires or tracks.

**Instruction:** Remove mud from tires and tracks by scraping. Any tool effective at removing mud is fine.

**Schedule:** NA

**Maintenance:** Upon incident. Apply roadway clean up per BMPs 2.3.3 & 2.3.4.

**Maintenance Personnel:** Perpetrating tradesmen

**Applicable Trades:** All tradesmen whose activity causes mud to stick to tires or tracks.

**Detail:** NA