**2.6.1 Trash Receptacle**

**Operation or Site Conditions:** All trades can generate light weight trash from the lunch box alone however, most will generate light weight trash as part of their operation. Light weight trash is the primary concern because it can blow off the site.

**Instruction:** I have provided (2) 60 gal trash receptacles with lids chained to post. All trades are required to use these or put your trash in your own vehicle. Do not fill receptacles with heavy weight trash see BMP 2.6.2 for heavy weight trash.

**Schedule:** Prior to land disturbance

**Maintenance:** Ensure lids are always closed. Dump when trash is spilling over.

**Maintenance Personnel:** Project Manager. All trades are expected to close lids.

**Applicable Trades:** All trades generating light weight trash of any kind

**Detail:** NA