**2.7.1 Storage Policy**

**Operation or Site Condition:** About 30 gallons of various liquids will be used for this project but will not be necessary until the foundation is complete. About 1000 lbs of various power will be necessary for this project and again will not be necessary until foundation and framing is complete.

**Instruction:** Store any liquids or powder supplies in the foundation for inside the building at all times.

**Schedule:** NA

**Maintenance:** NA

**Maintenance Personnel:** NA

**Applicable Trades:** Primarily, carpentry finishers, painters, brick masons or any tradesmen needing to store liquid or erodible construction materials not covered specific BMPs.

**Detail:** NA