**3.0 Spill Control Plan**

**Operations or Site Condition:** Spills can happen at any time. The project will extend into winter necessitating a plan that will work in freezing temperatures and snowy conditions.

**Instruction:**

1. Containment: Two 5 gal buckets with lids filled with sand are located at the low side of the project in the park strip, see site plan. Keep lid closed so the sand will stay dry. Wet sand will likely freeze solid. These are intended for containing flowing spills and absorbing spilled liquids, however, when site conditions allow dirt may also be used. You will need your own shovel.
2. Cleanup and Disposal: It will only take minutes to dam then absorb any liquid. Clean up immediately following the spill event. Dispose waste in BMP 2.6.5 unless the SDS directs otherwise.

**Installation Schedule:** Prior to any land disturbance

**Maintenance Requirements:** Replace as used

**Maintenance Personnel:** Project Manager

**Applicable Trades:** All

**Detail:** NA